|  |
| --- |
| **Directions - Gallery System Standard Allen Key Hooks**  |

|  |  |  |
| --- | --- | --- |
|

|  |  |
| --- | --- |
| **These Hooks are for use with both Gallery Clear Tape and the Gallery Stainless Steel Cable Hangers.**   |  |

**DIRECTIONS:** Slack off the screw using the key provided and feed the end of the clear tape (or stainless cable) through the hook body. Slide to the required position and tighten. **RECOMMENDED WEIGHT:**  On the Gallery Clear Tape Hangers 15kg per hook. On the Gallery Stainless Cable Hangers 20kg per hook. |



|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |