|  |
| --- |
| **Directions - Slimline Push-Button Hook** |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **These hooks are for use with Stainless Steel Cable Hangers only.**   |  |  |  | | --- | --- | --- | | **Directions:** Fit the stainless steel cable into the top of the hook.  To move the hook along the cable press the button on the top of the hook as shown. While the button is down the hook will move freely. The hook grips the cable when the button is released.  **Recommended Weight:** 14kg (30lbs) on one hook. |  | sl_pbhook_d1 |  |  |  |  | | --- | --- | --- | |  |  |  | |